{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价清单","index":0,"n_rows":70,"n_cols":7,"rows_kept":70,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[11,1,11,4],[12,0,12,6],[13,0,13,6],[24,1,24,3],[24,4,24,5],[25,0,25,6],[27,6,28,6],[29,6,30,6],[36,6,39,6],[44,6,45,6],[46,6,47,6],[49,6,50,6],[51,6,52,6],[61,1,61,3],[61,4,61,5],[62,1,62,3],[62,4,62,5],[65,4,65,5],[66,0,66,3],[66,4,66,5],[67,0,67,6]],"flags":["formulas_cached_only"]}
["集美全视野创业基地 充电项目招标清单"]
["一、设备部分"]
["1.主材清单"]
["序号","项目名称、特征","单位","数量","综合单价","合价","备注"]
[1,"800KVA箱式变电站（终端型）","台",1,null,null,"1.含运费\n2.S-20油浸式全铜变压器"]
[2,"800KVA箱式变电站（环网型）","台",1,null,null,"1.含运费\n2.S-20油浸式全铜变压器"]
[3,"壁挂式配电箱","台",1,null,null,"1.含运费\n2.含1个4P-C100A总开关、3个4P-C40A开关、6个2P-C16A开关等\n3.漏电保护系统"]
[4,"YJLHV-0.6/1KV 3*185+2*95","M",240,null,null,"1.含运费\n2.国标"]
[5,"YJLHV-0.6/1KV 4*150+1*70","M",350,null,null,"1.含运费\n2.国标"]
[6,"YJV 5*10mm","M",30,null,null,"1.含运费\n2.国标"]
[7,"YJV 3*6mm","M",100,null,null,"1.含运费\n2.国标"]
[null,"主材小计：(元）",{"$nulls":3},{"v":0,"d":"0.00"}]
["二、施工部分"]
["1、高压部分"]
["序号","项目名称、特征","单位","数量","综合单价/指导价\n","合价","备注"]
[1,"箱变安装","项",2,null,null,"含设备吊装卸货、二次搬运、开箱检查，本体就位，器身检查，垫铁及止轮器制作、安装，附件安装，接地、补漆，单体调试"]
[2,"箱变基础制作","项",2,null,null,"含接地"]
[3,"箱变调试、试验、送电","项",1]
[4,"设计费","项",1]
[5,"箱变围栏","米",50,null,null,"箱变围栏：1、材质：304不锈钢管"]
[6,"箱变标准化:(安全器具：绝缘手套、绝缘靴、操作棒、接地线\\标准化的图文内容：电缆及设备标书牌、二次接线图等)","项",2]
[7,"电缆敷设截面：ZC-YJV22-10kV-3*70","米",50,null,null,"电缆敷设费用（以实际供电答复为准）"]
[8,"热缩户内终端头制作，3*70mm2-120mm2","个",2,null,null,"高压电缆头制作（热缩套管，压接线鼻子、绝缘胶带、孔洞防火泥封堵）"]
[9,"协调费","项",1]
[null,"单项小计",null,null,{"v":0,"d":"0.00"}]
["1、低压部分"]
["序号","项目名称、特征","单位","数量","综合单价/指导价","合价","备注"]
[1,"地上砖砌电缆沟，宽1000，地上高300，（单排电缆沟一层支架，带圈梁)","m",40,null,null,"地上电缆沟砌筑（垫层、砌筑、水泥砂浆、回填、盖板、接地网，清运）"]
[2,"水泥井盖，角钢包边  厚度5CM","m",35]
[3,"砖砌电缆沟，内径：宽600*深500（单排电缆沟一层支架)","m",10,null,null,"地下电缆沟砌筑（垫层、砌筑、水泥砂浆、回填、盖板、接地网，清运）"]
[4,"水泥井盖，角钢包边  厚度5CM","m",8.75]
[5,"混凝土路面20cm，挖土断面：500*700mm（宽*深）","m",25,null,null,"1.原混凝土路面切缝破碎开挖\n2.原土回填夯实\n3.碎石10cm\n3.C25混凝土路面恢复10cm，最大粒径40mm\n4.清运"]
[6,"混凝土路面20cm，挖土断面：300*500mm（宽*深）","m",70,null,null,"1.原混凝土路面切缝破碎开挖\n2.原土回填夯实\n3.碎石10cm\n3.C25混凝土路面恢复10cm，最大粒径40mm\n4.清运"]
[7,"PVC管埋地敷设，规格：DN110，壁厚4mm","m",50]
[8,"PVC管埋地敷设，规格：DN75，壁厚3mm","m",45]
[9,"PVC管埋地敷设，规格：DN50，壁厚2mm","m",60]
[10,"电缆敷设：YJLHV 3*185+1*95","M",240,null,null,"电缆保护管敷设（配管、锯管、煨弯、管口处理、接管、埋设、接管口）"]
[null,"电缆敷设：YJLHV 4*150+1*70","M",350]
[11,"电缆敷设：YJV 5*10mm","M",30]
[12,"电缆敷设：YJV 3*6mm","M",100]
[13,"热缩终端头制作，185mm2内 五芯","套",64,null,null,"低压电缆头制作（热缩套管，压接线鼻子、绝缘胶带、孔洞防火泥封堵）"]
[14,"壁挂式配电箱安装","个",1]
[15,"480KW整流柜安装（含现场卸货）","个",4]
[16,"分体机终端安装（含现场卸货）","个",16]
[17,"C25砼浇筑基础，规格：1400*1150*600，高出地坪：200mm","座",1,null,null,"充电桩基础及箱体安装（人工挖基坑、基地夯实、浇筑混凝土垫层、浇筑混凝土基础、预埋件、回填土、箱体安装、固定预埋件、设备安装含接线）"]
[18,"C25砼浇筑基础，规格：600*300*600，高出地坪：200mm","座",2]
[19,"C25砼浇筑基础，规格：1400*1000*600，高出地坪：200mm","座",3,null,null,"1.与地上电缆沟一体式基础\n2.终端背靠背安装，共用基础\n3.充电桩基础及箱体安装（人工挖基坑、基地夯实、浇筑混凝土垫层、浇筑混凝土基础、预埋件、回填土、箱体安装、固定预埋件、设备安装含接线）"]
[20,"C25砼浇筑基础，规格：1000*600*300，高出电缆沟：200mm","座",7]
[21,"（充电桩、配电箱、箱变、电缆沟等）基础表面刷漆，黄黑相间800，右斜45°","项",1,null,null,"基础表面处理和美化"]
[22,"接地扁铁，热镀锌—40X4（箱变接地和充电桩接地网连接，）","米",80,null,null,"防雷接地（设计电阻<4Ω）"]
[23,"接地极（50*5*2500镀锌角钢）","根",12]
[24,"磷酸铵盐干粉灭火器（30公斤）手推式","组",2,null,null,"消防设施"]
[25,"磷酸铵盐干粉灭火器（2*5公斤）手提式","组",6]
[26,"砖砌1080*1080*1000，铸铁重型井盖","口","2",null,null,"手孔井和电缆工井（人工挖基坑、基地夯实、浇筑混凝土垫层、砌筑砖基础、四周抹灰、回填土、安装井盖）"]
[27,"车挡器安装（DN76*2000*3 钢管）","套",32,null,null,"车挡器安装（挖填土、基底夯实、钢管、混凝土、预埋板、检查、安装）"]
[28,"划车位线,宽150mm（热熔）","m",600,null,null,"含除线等所有工序"]
[29,"监控照明系统","套","1",null,null,"1、含400万POE红外网络枪型摄像机（4mm）8个、8路硬盘录像机\n2、监控专用硬盘4T一只\n3、8口全千兆云管理POE交换机\n4、照明设施9根含施工安装\n5、其他辅材弱电箱，电源线、网线等。\n6、施工。"]
[30,"休息室","项","1",null,null,"\n1、配置桌椅；\n2、配置1.5匹及以上空调；\n3、配置照明电源插座等；\n4、尺寸不小于6m*3m*2.5m"]
[31,"厕所","个","2",null,null,"1、配置独立开式厕所；\n2、配置洗手池；\n3、配置化粪池；\n4、配置照明冲水系统等；\n5、含引至最近污水井"]
[32,"道闸系统","套","1",null,null,"需与原有停车场道闸系统对接，需提供3年宽带，由施工方申请。"]
[33,"广告牌及流程牌采购及安装","项",1,null,null,"1、充电流程牌、充电指引牌安装2套（贴纸）\n2、立招（高*宽*厚2500mm*1095mm*175mm）基础及安装1套\n3、以实际设计为准"]
[null,"单项小计",null,null,{"v":0,"d":"0.00"}]
[null,"单项合计",null,null,{"v":0,"d":"0.00"}]
[1,"安全文明施工费","项",1,0.03,{"v":0,"d":"0.00"}]
[2,"税金（施工安装）","项",1,0.09,{"v":0,"d":"0.00"}]
[3,"施工部分合计","项",1,{"v":0,"d":"0.00"}]
["项目总计(一)+（二）",{"$nulls":3},{"v":0,"d":"0.00"},null,"含税"]
["注：最终报价以终版设计施工为准。"]
[null,"投标人："]
[null,"联系方式："]