{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":11,"rows_kept":16,"merged":[[0,0,0,10],[1,0,1,10],[2,0,2,10],[3,0,3,10],[4,0,4,10],[5,0,5,10],[6,0,6,10],[7,7,7,8],[8,7,8,8],[8,9,15,9],[8,10,15,10],[9,7,9,8],[10,7,10,8],[11,7,11,8],[12,7,12,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[13,6,15,6],[13,7,15,8]]}
["危险废物产生单位信息公开"]
["企业名称：厦门通士达照明有限公司"]
["环保负责人及电话：林利霞 0592-7263594"]
["危险废物产生规模：0-15吨"]
["危险废物贮存设施数量：暂存库 2 处"]
["危险废物贮存设施建筑面积（容积）：暂存库  30  平方米   "]
["危 险 废 物 信 息"]
["序号","废物名称","废物类别","废物代码","危险特性","产生环节","污染防治措施","去向 （处置单位）",null,"责任人","联系电话"]
[1,"医疗废物","HW01","841-001-01","感染性","医务室","防雨、防晒、防渗","委托有资质企业处置",null,"林利霞",13656010612]
[2,"废有机溶剂","HW06","900-404-06","易燃性、有毒性、反应性","机台清洗","防火、防渗、防雨、防晒、","委托有资质企业处置"]
[3,"废矿物油与矿物油废物","HW08","900-249-08","易燃性、有毒性","车间机台维护","防火、防渗、防雨、防晒","委托有资质企业处置"]
[4,"染料、涂料废物","HW12","900-299-12","有毒性","车间划线粉刷及组装喷码","防渗、防雨、防晒","委托有资质企业处置"]
[5,"有机树脂类废物","HW13","900-014-13","有毒性","组装车间灌胶","防渗、防雨、防晒","委托有资质企业处置"]
[6,"其他废物","HW49","900-041-49","有毒性、感染性","组装车间擦拭整灯、含密封胶容器、机台维修过程、活性碳设施过滤棉更换等产生","防渗、防雨、防晒","委托有资质企业处置"]
[{"$nulls":3},"900-045-49","有毒性","组装车间生产过程中损坏、研发样品"]
[{"$nulls":3},"900-039-49","有毒性","注塑、移印过程用于吸收废气产生的废活性炭"]